

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **DatasheetModel: KYBX-100-PM (PS/2 or USB)***(Rugged, Vandal Resistant Panelmount Keyboard)*The Stealth model KYBX-100-PM keyboard is an industrial grade panelmount keyboard housed in a rugged vandal resistant stainless steel enclosure and will stand up to harsh, wet and dirty environments. The KYBX-100-PM features 64 flat keys for easy cleaning, has an extended temperature range and is ideal for Kiosks and Public Access applications.Stealth.Com is an ISO 9001 recognized industry leader in the development of specialized computers and peripherals for industrial and commercial markets. For unsurpassed performance and reliability contact Stealth today to discuss your application with one of our product specialists. Toll Free: 1-888-STEALTH (1-888-783-2584) or International 905-264-9000. |   |

|  |  |  |
| --- | --- | --- |
| **Product Photo** | http://www.stealth.com/images/dotline_divider.jpg | **Keyboard Features** |
| http://www.stealth.com/images/KYBX-100-PM_front1_medium.jpg*(click on image for a larger picture)*

|  |
| --- |
| **Ordering Information** |
|  |

 | * Rugged Stainless Steel, Vandal Resistant
* 64 Flat Keys, Sealed and easily cleanable
* -20 to +60C (-4 to 140F) Temperature Range
* 5 Million Actuations Expected life
* Full Travel, Tactile Laser Etched Keys
* Panel mount enclosure
* Includes 5.75' USB or PS/2 cable
* Dimensions: (W-H-D)Unit: 12.99" x 4.72" x 0.78"330mm x 120mm x 20mm295mm x 105mm (front panel)330mm x 120mm (back panel)

|  |
| --- |
| **Technical Information** |
|   |

 |
| **Technical Specifications** | http://www.stealth.com/images/dotline_divider_grey.jpg |   |
| * **Industrial Approvals**NEMA 4, 4X, IP65 (from top of panel)RoHS Compliant
* **Key Switch**Material/Style: Brushed stainless steel buttonsLife: >5 million actuationsTravel: 0.45mm (0.017")Contact: Gold-on-Gold key switch PCBActuation Force: 2.0N+/-0.1N
* **Power**Supply Voltage: +5V DC +/-5%Current Rating: Approx. 20mA
* **Temperature Range**Operating: -20C to +60C (-4F to +140F)Storage:-30C to +70C (-22F to +158F)
* **Humidity**30-90%
* **Other Environmental**Atmospheric pressure: 60-106Kpa.Saline mist: 96 hours, IEC 60512-6Damp heat test at + 40oC: 21 days, IEC 60512-6Dry heat test at + 85oC: 10 days, IEC 60512-6
 |  | * **Housing**Rugged, Vandal Resistant Stainless Steel casing
* **Dimensions**(W-H-D)Unit: 12.99" x 4.72" x 0.78"330mm x 120mm x 20mm295mm x 105mm (front panel)330mm x 120mm (back panel)
* **Weight**Unit: 3.0 lbs (1.36 kg)
* **Cable**Length: 5.75 feet (1.75m)Design: Single USB1.1Cable
* **Compatibility**USB 1.1/2.0 Keyboard/Mouse:Compatible with all Windows Operating Systems
* **Warranty:**1 Year Limited Warranty
* **Model Numbers**KYBX-100-PM-USB (USB Interface)KYBX-100-PM-PS/2 (PS/2 Interface)
 |
| *NOTE: Specifications subject to change without notice.* |

 |